Serial communication

Communication baud rate: 9600 without parity, data bit is 8, stop bit is 1;

letter of agreement:

OC (01, XXX) Electric cylinder one position control

OC (02, XXX) Electric cylinder two position control

OC (03, XXX) pan electric cylinder position control

XXX means 000-255,000 means reset, 001-255 means position stroke (recommended use range 010-200)

Send at least 10ms interval for each instruction to filter out duplicate instructions

Left rope: I (1, xxx)

Pull rope on the right: I (2, xxx)

Wind authority: OD (00,00)

Fan opening: OD (00,04)

Fan opening: OD (00,08)